|  |  |  |  |
| --- | --- | --- | --- |
| Title | **Demonstrate knowledge of vehicle body frame construction and body panelling in the coachbuilding industry** | | |
| Level | **4** | **Credits** | **4** |

|  |  |
| --- | --- |
| Purpose | People credited with this unit standard are able to demonstrate knowledge of vehicle body frame construction in the coachbuilding industry, and vehicle body panelling in the coachbuilding industry. |

|  |  |
| --- | --- |
| Classification | Motor Industry > Coachbuilding |

|  |  |
| --- | --- |
| Available grade | Achieved |

**Guidance Information**

1. Evidence presented for assessment against this unit standard must be consistent with safe working practices and be in accordance with applicable service information, company requirements and legislative requirements. This includes the knowledge and use of suitable tools and equipment.
2. Legislation, regulations and/or industry standards relevant to this unit standard include but are not limited to the current version of the Health and Safety at Work Act 2015 and any subsequent amendments or replacements.
3. Definitions

*Company requirements* refers to instructions to staff on policy and procedures that are available in the workplace. These requirements may include – company policies and procedures, work instructions, product quality specifications and legislative requirements.

*Service information* refers to information such as technical information for a vehicle, machine, or product detailing operation; installation and servicing procedures; manufacturer instructions; technical terms and descriptions; and detailed illustrations.

**Outcomes and performance criteria**

**Outcome 1**

Demonstrate knowledge of vehicle body frame construction in the coachbuilding industry.

**Performance criteria**

1.1 Types of body construction are identified.

Range bus, Luton, curtainside, refrigerated, demountables, motor home, tipping bodies, flat deck.

1.2 Types and purpose of framing are identified.

Range chassis, waist rails, cant rails, pillars, skirt rails, crown rails (roof rails), stress panels, roof bows.

1.3 Frame attachments are identified.

Range bracing, gussets, brackets.

1.4 Methods of assembling frames are identified.

Range welding, bolts, rivets, approved fasteners.

1.5 Methods of aligning and checking the alignment of frames are identified.

1.6 Painting and anti-corrosion procedures are identified.

1.7 Land Transport Rules covering vehicle body construction are identified.

Range trucks, trailers, passenger service vehicles, vans;

kerb weight, tare weight, gross weight.

**Outcome 2**

Demonstrate knowledge of vehicle body panelling in the coachbuilding industry.

**Performance criteria**

2.1 Types and characteristics of body panels are identified.

Range aluminium, panel steel, stainless steel, plastic, glass reinforced plastic.

2.2 Methods of attaching panelling to frame work are identified.

Range adhesive bonding, rivet bonding, mechanical fastenings, welding.

|  |  |
| --- | --- |
| Planned review date | 31 December 2025 |

**Status information and last date for assessment for superseded versions**

| Process | Version | Date | Last Date for Assessment |
| --- | --- | --- | --- |
| Registration | 1 |  |  |
|  | 2 |  |  |
|  | 3 |  |  |
|  | 4 |  | 31 December 2023 |
| Review | 5 |  | N/A |

|  |  |
| --- | --- |
| Consent and Moderation Requirements (CMR) reference | 0014 |

This CMR can be accessed at <http://www.nzqa.govt.nz/framework/search/index.do>.

**Comments on this unit standard**

Please contact MITO New Zealand Incorporated [info@mito.org.nz](mailto:info@mito.org.nz) if you wish to suggest changes to the content of this unit standard.